**Pottery Painting with Acrylics**

1. Wipe off the bisque piece with a damp sponge before painting. Do not get it too wet; you are just trying to remove the dust.
2. Paint your piece, using 2 to 3 coats for each color. Let the paint dry between coats.
3. When the piece is finished and the paint is completely dry, paint on one (1) coat of poly acrylic for shine. Let dry.
4. No is firing required with acrylics\*\*.

\*\* Acrylic paints are not food-safe.

**Pottery Painting with Glaze**

1. Wipe off the bisque piece with a damp sponge before painting. Do not get it too wet; you are just trying to remove the dust.
2. Paint your piece, using 2 to 3 coats for each color. Let the paint dry between coats.
3. When the paint is completely dry, fill out the enclosed contact form and drop off at the studio for firing.
4. Firing is required with glaze and it will be food-safe.